**RFQ FOR INNER AND OUTER LINERS**:

QUANTITIES ARE MINIMUM 1400 AND MAXIMUM 4400 PER YEAR FOR 5 YEARS.

**Particulate Inner Liner**

Extended Description: Pre-production samples, 5 each, are

required 30 days after award.  Particulate

Inner Liner shall be IAW ASTM F1267, Type II, (Expanded and

Flattened) Class 2, Grade A, .030 STK. All specifications IAW

Drawing 63-320-ME-3013

**Particulate Outer Liner**

Extended Description: Pre-production samples, 5 each, are

required 30 days after award. Particulate

Outer Liner shall be IAW ASTM F1267, Type II, (Expanded and

Flattened) Class 2, Grade A, .030 STK. All specifications IAW

Drawing 63-320-ME-3013

Quantity range that needs to be quoted is :      500-1500

                                                                         1501-2200

                                                                         2201-3200

                                                                         3201-4400

This would be a multiple year requirement also.

Thanks in advance.  I need a quote no later than 1pm tomorrow 1/7/15.

PLEASE EMAIL ME AT BRENCOSUPPLY2@GMAIL.COM . IF YOU FEEL YOU CAN QUOTE, I NEED TO GET A NDA SIGNED AND SEND DRAWINGS ASAP

THANKS

PAULA GONZALEZ